Open topic with navigation

TIBCO GridServer® 7.1.0

# Communication

The GridServer architecture combines the central control of a hub and spoke architecture with the efficient communication of a peer-to-peer architecture. This is made possible by the flexibility in configuring communication between the Broker, Engines, and Drivers.

Engines and Drivers communicate with Brokers using lightweight transaction messages. Direct Data Transfer (DDT) enables Engines and Drivers to exchange work data directly. This peer-to-peer communication eliminates any “heavy lifting” between the Broker and clients, improving its performance.

DDT can be disabled in situations where network layout requires all communication to go through a central point like a Broker. This causes both transaction messages and data to be transferred through the Broker, creating a more traditional hub and spoke architecture between Brokers and clients.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO GridServer®

Copyright © 2001-2022. TIBCO Software Inc. All Rights Reserved.