Open topic with navigation

TIBCO GridServer® 7.1.0

# Configuration Issues

# Installation on Machines With Multiple Network Adapters

In some network configurations, on a machine with more than one network interface, a GridServer component can default to using the incorrect interface. You can configure the component to use the correct interface as follows:

| • | Drivers To configure the Driver to use a different network interface, edit the `driver.properties` file and set the `DSLocalIPAddress` property to the IP number of the correct interface. For example:

`DSLocalIPAddress=192.168.12.1`

| • | Engines To configure the Engine to use a different network interface, select the Engine Configuration used by the Engine on the Engine Configuration page, and set the Net Mask value under the File Server heading to match the network range on which to run the Engine.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO GridServer®

Copyright © 2001-2022. TIBCO Software Inc. All Rights Reserved.