Open topic with navigation

TIBCO GridServer® 7.1.0

# Configuring Engines With Multiple Network Adapters

In some network configurations, the host running an Engine can have more than one physical or logical network interface. When the Engine starts, it checks what IP address is in use and uses it to advertise its file server location. In cases where there is more than one network interface, it's possible for the Engine to pick the wrong one. To remedy this it is possible to force the Engine to choose a specific interface. To configure the Engine to use a different network interface, select the Engine Configuration it uses on the Engine Configuration page, and set the Net Mask value under the File Server heading to match the network range on which to run the Engine.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO GridServer®

Copyright © 2001-2022. TIBCO Software Inc. All Rights Reserved.