Open topic with navigation

TIBCO GridServer® 7.1.0

# Configuring Multi-Interfaced Drivers

In some network configurations, on a PC with more than one network interface, a Driver might default to using the incorrect interface, resulting in the Engines using the incorrect IP address for the Driver's file server. To configure the Driver to use a different network interface, set the `DSLocalIPAddress` property to the IP number of the correct interface. For example:

    DSLocalIPAddress=192.168.12.1

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO GridServer®

Copyright © 2001-2022. TIBCO Software Inc. All Rights Reserved.