Open topic with navigation

TIBCO ActiveSpaces® 4.8.0

# Query Capacity

Mirror grids must be provisioned appropriately for the load expected of them. A data grid that serves as both a read replica and a DR grid, must be capable of handling the total of both the normal load when being used as a read replica and the normal load of the primary grid, in case it is changed to the primary grid.

Copyright © 2009-2022. Cloud Software Group, Inc. All Rights Reserved.