Open topic with navigation

TIBCO ActiveSpaces® 4.8.0

# Configuring a Proxy with Static Mirroring Host and Port

To set up disaster recovery, one proxy on the primary grid and one proxy on each mirror grid must be configured to use a static mirroring host and port. A static mirroring host and port uses an FTL static TCP transport to listen for mirroring operations.

To set static mirroring, configure the following properties:

- `proxy_mirroring_static_listen_port`
- `proxy_mirroring_static_listen_host`

Procedure
1. The following commands help you set up static mirroring host and port on a primary and mirror grid.

       tibdg -g grid1 proxy create dr_p1 proxy_mirroring_static_listen_port=9001 proxy_mirroring_static_listen_host=10.0.0.1

       tibdg -g grid2 proxy create dr_p2 proxy_mirroring_static_listen_port=9001 proxy_mirroring_static_listen_host=10.0.0.2

Copyright © 2009-2022. Cloud Software Group, Inc. All Rights Reserved.