Open topic with navigation

TIBCO ActiveSpaces® - Enterprise Edition 5.0.0

# Query Capacity

Mirror grids must be provisioned appropriately for the load expected of them. A data grid that serves as both a read replica and a DR grid, must handle the total of both the normal load when being used as a read replica and the normal load of the primary grid, in case it is changed to the primary grid.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO ActiveSpaces® - Enterprise Edition

Copyright © 2009-2025. Cloud Software Group, Inc. All Rights Reserved.