Open topic with navigation

TIBCO ActiveSpaces® - Enterprise Edition 5.0.0

# Configuring a Proxy with Static Mirroring Host and Port

To set up disaster recovery, configure one proxy on the primary grid and one proxy on each mirror grid to use a static mirroring host and port. A static mirroring host and port uses an FTL static TCP transport to listen for mirroring operations.

To set static mirroring, configure the following properties:

- `proxy_mirroring_static_listen_port`
- `proxy_mirroring_static_listen_host`

Procedure
1. The following commands help you set up a static mirroring host and port on a primary and mirror grid.

       tibdg -g grid1 proxy create dr_p1 proxy_mirroring_static_listen_port=9001 proxy_mirroring_static_listen_host=10.0.0.1

       tibdg -g grid2 proxy create dr_p2 proxy_mirroring_static_listen_port=9001 proxy_mirroring_static_listen_host=10.0.0.2

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO ActiveSpaces® - Enterprise Edition

Copyright © 2009-2025. Cloud Software Group, Inc. All Rights Reserved.