# Active-Active Configuration

In an active-active configuration, you may specify selectors on either or both servers. If you specify `outgoing_topic` selector S1 for topic T on server A, and `incoming_topic` selector S2 for T on server B, then the effective selector for T on the route from A to B is (S1 AND S2).

See also Active and Passive Routes.

Copyright © Cloud Software Group, Inc. All rights reserved.