# TIBCO FTL Transport Parameters

The parameters listed here enable the EMS server to connect to a TIBCO FTL realm service using transports configured in the `transports.conf` file.

Note: The EMS server creates a single FTL event queue that is used for all EMS transports for FTL configured in the `transports.conf` file.

The discard parameters set here are global, and refer to the EMS server and its single FTL event queue. These settings cannot be set for individual transports.

For more information, see Interoperation with TIBCO FTL.

Copyright © Cloud Software Group, Inc. All rights reserved.