# Transports

Enable or disable transports between the TIBCO Enterprise Message Service server and TIBCO FTL, TIBCO Rendezvous, and TIBCO SmartSockets by clicking the relevant check boxes.

Note: In order to enable a transport type, you must also set the Module Path field on the Server Properties page.

Transport configuration fields, including the Configured Transports index screen, are available only when transports are enabled.

## FTL Transports

Check the Enable FTL Transports check box to enable these transport types, then use the Configured Transports index screen to edit or create a new FTL transport definition.

When adding or editing a transport definition in the Configured Transports index screen, the fields available on the Transport properties page change depending on the Transport Type selected. When FTL is selected for this field, the fields shown correspond to the relevant parameters in the `transports.conf` configuration file. See also the section on "Transport Definitions" in the TIBCO Enterprise Message Service User’s Guide.

## RV and RVCM Transports

Check the Enable RV and RVCM Transports check box to enable these transport types, then use the Configured Transports index screen to edit or create a new RV transport definition.

The fields available on the Transport properties page change depending on the Transport Type selected. When RV or RVCM are selected for this field, the fields shown correspond to the relevant parameters in the `transports.conf` configuration file. See also the section on "Transport Definitions" in the TIBCO Enterprise Message Service User’s Guide.

## SmartSockets Transports

Check the Enable SmartSockets Transports check box to enable these transport types.

When adding or editing a transport definition in the Configured Transports index screen, the fields available on the Transport properties page change depending on the Transport Type selected. When SmartSockets is selected for this field, the fields shown correspond to the relevant parameters in the `transports.conf` configuration file. See also the section on "Transport Definitions" in the TIBCO Enterprise Message Service User’s Guide.

The SmartSockets Config Directory field that appears corresponds to the related TIBCO FTL Transport Parameters setting in the `tibemsd.conf` configuration file.

Copyright © Cloud Software Group, Inc. All rights reserved.