Collapse All Expand All Members: Show All Members: Filtered Members: Filtered Members: Filtered

Include Protected Members
Include Inherited Members

.NET Framework Class Library
Tibems Class See Also

[TIBCO.EMS .NET client library 5.1 documentation]

The Tibems type exposes the following members.

# Fields

| Name | Description
--- | --- | ---
| DEFAULT_FACTORY_PASSWORD | Defines the name of the ConnectionFactory property specifying default user password set for Connections created by the factory
| DEFAULT_FACTORY_USERNAME | Defines the name of the ConnectionFactory property specifying default user name set for Connections created by the factory
| FACTORY_CONNECT_ATTEMPT_COUNT | Defines the name of the ConnectionFactory property specifying the maximum iterations a client program will go through its URL list until it establishes its first connection to an EMS server.
| FACTORY_CONNECT_ATTEMPT_DELAY | Defines the name of the ConnectionFactory property specifying the interval between iterations a client program will try to establishe its first connection to an EMS server.
| FACTORY_CONNECT_ATTEMPT_TIMEOUT | Defines the name of the ConnectionFactory property specifying the maximum amount of time a client program will wait for the connection to be established to an EMS server This property is defined as String "TIBCO.EMS.connect.attempttimeout".
| FACTORY_LOAD_BALANCE_METRIC | Defines the name of the ConnectionFactory property specifying the load balancing metric to be used by the factory.
| FACTORY_LOAD_BALANCE_METRIC_BYTE_RATE | Indicates that the connection factory load balances connections across multiple servers by creating a connection to the server with the lowest total byte rate (input and output).
| FACTORY_LOAD_BALANCE_METRIC_CONNECTIONS | Indicates that the connection factory load balances connections across multiple servers by creating a connection to the server with the fewest number of connections.
| FACTORY_LOAD_BALANCE_METRIC_NONE | Indicates that no load balancing metric has been set for the connection factory.
| FACTORY_MULTICAST_DAEMON | Defines the name of the ConnectionFactory property specifying the port of the multicast daemon used by MessageConsumers subscribed to multicast-enabled topics. This property is defined as String "TIBCO.EMS.multicast.daemon".
| FACTORY_MULTICAST_ENABLED | Defines the name of the ConnectionFactory property specifying whether MessageConsumers subscribed to a multicast-enabled topic are to receive messages over multicast or unicast. This property is defined as String "TIBCO.EMS.multicast.enabled".
| FACTORY_RECONNECT_ATTEMPT_COUNT | Defines the name of the ConnectionFactory property specifying the maximum iterations a client program will try to re-establish a connection to an EMS server after losing previous connection.
| FACTORY_RECONNECT_ATTEMPT_DELAY | Defines the name of the ConnectionFactory property specifying the interval between reconnection attempts.
| FACTORY_RECONNECT_ATTEMPT_TIMEOUT | Defines the name of the ConnectionFactory property specifying the maximum amount of time a client program will wait for the connection to be re-established to an EMS server This property is defined as String "TIBCO.EMS.reconnect.attempttimeout".
| JMS_TIBCO_CM_PUBLISHER | Provider-specific message property which may be set if imported message has been published by TIBCO Rendezvous Certified Messaging application.
| JMS_TIBCO_CM_SEQUENCE | Provider-specific message property which may be set if imported message has been published by TIBCO Rendezvous Certified Messaging application.
| JMS_TIBCO_COMPRESS | Provider-specific message property which is set by the application if this message should be compressed before it is sent to the server.
| JMS_TIBCO_DISABLE_SENDER | Provider specific message property which may be set to prevent the server from including the user name into message when sending this message to consumers.
| JMS_TIBCO_IMPORTED | Provider-specific message property which is set by the provider if the message has been imported from an external message service, such as TIBCO Rendezvous or TIBCO SmartSockets.
| JMS_TIBCO_MSG_EXT | Provider-specific message property which is set by the provider or the application when message extensions are used.
| JMS_TIBCO_MSG_TRACE | Provider-specific message property which is set by the provider or the application when message extensions are used.
| JMS_TIBCO_PRESERVE_UNDELIVERED | Provider-specific message property which is set by the application if this message should be placed into special system queue in case it could not be delivered.
| JMS_TIBCO_SENDER | Provider-specific message property which may be set in a received message if message has been sent on a destination with sender name property. When set in the message, the property value is a String specifying the name of the user who sent this message.
| JMS_TIBCO_SS_SENDER | Provider-specific message property which is set if imported message has been published by TIBCO SmartSockets application.
| NPSEND_CHECK_ALWAYS | Defines mode when producer always checks result of sending a NON_PERSISTENT message. See SetNPSendCheckMode(MessageProducer, Int32).
| NPSEND_CHECK_AUTH | Defines mode when producer checks result of sending a NON_PERSISTENT message only when server authorization is enabled. See SetNPSendCheckMode(MessageProducer, Int32).
| NPSEND_CHECK_DEFAULT | Defines default check mode for sending a NON_PERSISTENT messages. See SetNPSendCheckMode(MessageProducer, Int32).
| NPSEND_CHECK_NEVER | Defines mode when producer never checks result of sending a NON_PERSISTENT message. See SetNPSendCheckMode(MessageProducer, Int32).
| NPSEND_CHECK_TEMP_AUTH | Defines mode when producer checks result of sending a NON_PERSISTENT message when sending into temporary destination or if server authorization is enabled. See SetNPSendCheckMode(MessageProducer, Int32).
| NPSEND_CHECK_TEMP_DEST | Defines mode when producer checks result of sending a NON_PERSISTENT message only when sending into temporary destination. See SetNPSendCheckMode(MessageProducer, Int32).
| PROP_CLOSE_IN_CALLBACK | Defines the name of the provider property controlling if a MessageConsumer.close(), Session.close() or Connection.close() methods can be called in the MessageListener callback.
| PROP_CONNECT_ATTEMPT_TIMEOUT | Defines the name of the System Property controlling the maximum time for the connections to connect to the server. When too many clients connect to the same server, the server may not be able to accept all connections at the same time or may run out of system resources. This parameter specifies the amount of time a client is willing to wait for a connection to be established. Internally the client library will tear down any hung connections (either because of non-availiblity of system resources or some other EMS server problem) after this timeout. The value of this property in an integer and is in seconds. This property is defined as String "tibco.tibjms.connect.attempt.timeout".
| PROP_CONNECT_ATTEMPTS | Defines the name of the provider property controlling the number of attempts the connections make to connect to the server.
| PROP_DAEMON_DISPATCHER | Defines the name of the provider property controlling the type of Session dispatcher threads
| PROP_FT_SWITCH_EXCEPTION | Defines the name of the provider property controlling if ExceptionListener set on the Connection should be called during fault-tolerant switch.
| PROP_MESSAGE_ENCODING | Defines the name of the System Property setting the global encoding name for String values in the message properties and data fields.
| PROP_MULTICAST_DAEMON | Defines the name of the System Property specifying the port on which EMS clients will connect to the multicast daemon. This property is defined as String "tibco.tibjms.multicast.daemon".
| PROP_MULTICAST_ENABLED | Defines the name of the System Property specifying whether multicast is enabled or disabled for this EMS client. This property is defined as String "tibco.tibjms.multicast.enabled".
| PROP_PING_INTERVAL | Defines the name of the System Property setting the ping interval for inactive connections.
| PROP_RECONNECT_ATTEMPT_TIMEOUT | Defines the name of the System Property controlling the maximum time for connections to reconnect to the backup server during the fault-tolerant switch. This property is similar to PROP_CONNECT_ATTEMPTS_TIMEOUT. The difference is that it may be necessary to use different parameters during reconnect than during the initial connect. Initial connect of the clients to the server is normally distributed in time and there are less chances of the server exceeding its maximum accept queue. During fault-tolerant switch, all connected clients automatically try to reconnect to the backup server, approximately at the same time. When the number of connections is large, it may require more reconnect time to reconnect than the initial connect. The value of this property is an integer in seconds. This property is defined as String "tibco.tibjms.reconnect.attempt.timeout".
| PROP_RECONNECT_ATTEMPTS | Defines the name of the provider property controlling the number of attempt the connections make to reconnect to the backup server during the fault-tolerant switch.
| PROP_SOCKET_RECEIVE | Defines the name of the provider property setting the size of the socket receive buffer size in kilobytes for client connections.
| PROP_SOCKET_SEND | Defines the name of the provider property setting the size of the socket send buffer size in kilobytes for client connections.

# See Also

Tibems Class
TIBCO.EMS Namespace