> Configuring C and COBOL Clients for Fault-Tolerant Connections
> When connecting a fault-tolerant client to EMS, you must specify two or more EMS servers, as described in Configuring Clients for Fault-Tolerant Connections in the TIBCO Enterprise Message Service User’s Guide.
> C clients list the primary and backup server URLs in the brokerURL argument to a connection constructor, separated by a comma.
> Example
> In this example, the first server is tcp://server0:7222, and the second server is tcp://server1:7344 (if first server is not available).
> tibemsConnection_Create(
> &connection,
> "tcp://server0:7222,
> tcp://server1:7344",
> NULL, "admin", NULL );

Copyright © TIBCO Software Inc. All Rights Reserved.