Copyright © TIBCO Software Inc. All Rights Reserved

> tibemsMsg_SetPriority
> Function
> Purpose
> Set the priority header of a message.
> C Declaration
> tibems_status tibemsMsg_SetPriority(
> tibemsMsg message,
> tibems_int value );
> COBOL Call
> CALL "tibemsMsg_SetPriority"
> USING BY VALUE message,
> BY VALUE value,
> RETURNING tibems-status
> END-CALL.

> | message has usage pointer.

> Parameters

> Parameter | Description
> message | Set the priority of this message.
> value | Set the priority to this value.

> Remarks
> Sending calls set the priority header automatically. The JMS specification defines this call for symmetry.
> Sending calls record the priority of a message in this header, based on either a property of the producer, or on a parameter to the send call.
> The JMS specification defines ten levels of priority value, from zero (lowest priority) to 9 (highest priority). The specification suggests that clients consider 0–4 as gradations of normal priority, and priorities 5–9 as gradations of expedited priority.
> Priority affects the order in which the server delivers messages to consumers (higher values first). The JMS specification does not require all providers to implement priority ordering of messages. (EMS supports priorities, but other JMS providers might not.)
> See Also
> tibemsMsg_GetPriority on page 44
> tibemsMsgProducer_GetPriority on page 182
> tibemsMsgProducer_SetPriority on page 192

Copyright © TIBCO Software Inc. All Rights Reserved