Copyright © TIBCO Software Inc. All Rights Reserved

> tibems_SetMulticastEnabled
> Function
> Purpose
> Set whether message consumers subscribed to multicast-enabled topics in the EMS client application will receive messages over multicast.
> C Declaration
> tibems_status tibems_SetMulticastEnabled(
> tibems_bool enabled);
> Parameters

> Parameter | Description
> enabled | When true, multicast is enabled for the client. When false, multicast is disabled and the client application will receive all messages over TCP.

> Remarks
> When enabled, message consumers subscribed to a multicast-enabled topic will receive messages over multicast. By default, multicast is enabled.
> tibems_SetMulticastEnabled overrides both the EMS server and factory settings that enable multicast.
> See Also
> tibemsConnectionFactory_SetMulticastDaemon on page 272
> multicast and multicast_daemon_default server parameters in the TIBCO Enterprise Message Service User’s Guide

Copyright © TIBCO Software Inc. All Rights Reserved