Copyright © TIBCO Software Inc. All Rights Reserved

> tibems_SetMulticastDaemon
> Function
> Purpose
> Sets the port on which the EMS client will connect to the multicast daemon.
> C Declaration
> tibems_status tibems_SetMulticastDaemon(
> const char* port);
> Parameters

> Parameter | Description
> port | The multicast daemon port that connections created in this application will connect to.

> Remarks
> A connection to the multicast daemon is required when multicast is enabled and a consumer is subscribed to a multicast-enabled topic. Setting the port with this method will override the default port supplied by the server and any port specified in a connection factory for all connections in the application.
> See Also
> tibemsConnectionFactory_SetMulticastDaemon on page 272
> tibems_SetMulticastEnabled on page 402
> Chapter 13, Using Multicast, in the TIBCO Enterprise Message Service User’s Guide

Copyright © TIBCO Software Inc. All Rights Reserved