Open topic with navigation

# Authenticating to FTL Server

FTL server can be configured with one or more authentication providers, allowing FTL server to understand basic authentication, mTLS authentication, oauth2 authentication, or all three. When accepting incoming connections, FTL server can accept different authentication modes for different connections, as long as an appropriate auth provider is configured.

In addition, each client and FTL server must be configured to authenticate itself to FTL servers. When making a connection to an FTL server, the client or server must choose exactly one of the possible authentication modes (basic, mTLS, or oauth2). For FTL server, this configuration (for outgoing connections) is independent of the auth provider configuration (for incoming connections). For more information, see FTL Server Configuration Parameters

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.