Open topic with navigation

# Static TCP Transport

A static TCP transport communicates over a set of dedicated connections. A static TCP transport can be server-based or peer-to-peer.

Note: In most cases it is simpler and more flexible to use dynamic TCP transports (see Dynamic TCP Transport).

Static TCP is a connection-oriented protocol. Its transport definitions are inherently fragmentary. You must define at least two complementary transport definitions to establish a bus. For more information, see Pair Connections.

Although an individual static TCP connection links exactly two host computers, you can combine several connections into a bus with a more complex topology (see Assembling Larger Topologies from Pair Connections).

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.