Open topic with navigation

# Shared Memory Transports and One-to-Many Non-Blocking Send

Shared memory transports buffer message data from one-to-many send calls in the shared memory segment itself, rather than in a backlog buffer in process memory.

To counteract dataloss in this situation, enlarge the Segment Size of the shared memory segment in the transport definition, rather than increasing the backlog buffer size.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.