Open topic with navigation

# Core Servers

A core server is an FTL server to which FTL clients connect.

A core server provides an explicitly configured realm service, which is essential for client operations.

A cluster of core servers can cooperate for fault tolerance, or a single core server can operate solo. It is best practice to specify an odd number of core servers. You must specify at least one core server.

Specify the set of core servers in the core.servers map within the globals section of the FTL server configuration file.

    globals:
        core.servers:
            ftl1: host1:8585
            ftl2: host2:8585
            ftl3: host3:8585

Specify the host and port location of each core server in this map.

The host can specify a host computer or an interface of a host computer.

The port specifies the port for all communications with the server. Even if an FTL server provides several services, network administrators need open only one port. The server automatically multiplexes the request stream to its services. The default port number is 8585.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.