Open topic with navigation

# Asymmetric Multicast Topologies

In this example of an asymmetric multicast topology, three sending applications on the left side can send one-to-many messages to three receiving applications on the right side. You can easily generalize this example to any number of senders and receivers, and the number of senders and receivers need not be the same.

Configure these definitions:

- Transport TS specifies send group G1.
- Transport TL specifies listen group G1.
- Connectors in the senders (left) bind TS to carry the send ability.
- Connectors in the receivers (right) bind TL to carry the receive ability.

  Figure 30: Asymmetric Multicast, Bipartite Graph

Notice that all these processes use only two different transport definitions, TS and TL, to join the bus, reflecting their opposite roles as either senders or receivers.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.