Open topic with navigation

# Multicast Retransmission Suppression

The high volume of retransmission requests from chronically slow or lossy receivers can overwhelm publishing applications and even overwhelm the entire network. Receiver loss can result from faulty network hardware, oversubscribed applications, or underpowered host computers.

The retransmission suppression feature can detect lossy receivers and suppress their retransmission requests. Administrators can set a receiver loss threshold. If the percentage of lost packets between any pair of multicast subscriber and publisher exceeds this threshold, then the transport suppresses all retransmission requests from that subscriber to that publisher.

To configure this threshold, see Multicast Transport: Parameters Reference.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.