Open topic with navigation

# Transport Bridge Restrictions

Although transport bridges are flexible, these restrictions apply.

- Transport bridges support only bidirectional transports. For example, a bridge cannot support a multicast transport configured with a send group but without a listen group, nor vice versa.
- Transport bridges support only non-blocking transports. A transport that blocks could impede data flow through the bridge.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.