Open topic with navigation

# Transport Bridge to Extend beyond a Transport

You can use a transport bridge to extend the capabilities of a transport.

For example, in the following diagram, a publisher communicates with several subscribers on a single host computer using a shared memory transport T1. You can communicate with subscribers on other computers across a LAN by configuring a multicast transport T2, and a transport bridge between T1 and T2. The transport bridge must run on the computer that hosts the shared memory segment of T1.

Figure 45: Transport Bridge: Extending Capabilities

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.