Open topic with navigation

# Shared Memory Transport

Endpoints in programs that run on the same host computer can communicate using a shared memory transport. Shared memory transports are peer-to-peer transports that communicate at high speeds and exhibit very low latency.

Shared memory transports are an excellent strategy for fast communication among processes on multi-core hardware.

Shared memory transport definitions are inherently unitary.

## Topology

The natural topology of a shared memory bus is the mesh (complete graph) of all its runtime transports. All runtime transports can use the bus for both sending and receiving operations. When appropriate, you can configure connectors to artificially limit the abilities that an endpoint may use.

## Non-Blocking Send

See Shared Memory Transports and One-to-Many Non-Blocking Send.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.