Open topic with navigation

# Receive Spin Limit

Receive spin limit is an advanced parameter of transports. If you understand the role of threads in inbound message delivery, you can use it to eliminate a potential source of latency by increasing the CPU resources dedicated to inbound delivery.

Warning: Do not adjust the Receive Spin Limit except to achieve specific and well-defined performance objectives. Do not adjust unless you thoroughly understand all of the material about this topic.

For an introduction to message delivery, see “Inbound Message Delivery” in TIBCO FTL Development.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.