Open topic with navigation

# Multicast Transport (mcast)

A multicast transport is a peer-to-peer transport that carries reliable multicast communication among endpoints on many host computers. Multicast transports are efficient for high fan-out communication across a LAN.

Multicast transports excel at one-to-many communications.

Multicast transports use a negative acknowledgment protocol for reliable message transfer.

Multicast transports can also support one-to-one communications. For example, servers can send one-to-one replies to individual clients (that is, requestors). For configuration details, see Configuring Multicast Inbox Communication.

Multicast transports can filter messages by subscriber interest.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.