Open topic with navigation

# Static TCP Transport: Parameters Reference

The following tables describe the parameters specific to static TCP transports and secure static TCP transports in the configuration interface.

For web API access to transport definitions, see Transport Definition Objects.

## Connection List

You must specify at least one pair connection triplet: host, port, and initialization mode.

In the web API, the `hosts` attribute contains a collection of these triplet objects.

GUI Parameter | JSON Attribute | Description
--- | --- | ---
Host | `host` | Required. For the host, specify an interface either as a host name or as an IP address. Asterisk (*) is a special value, which designates all interfaces on the host computer (analogous to INADDR_ANY, but limited to TCP interfaces). This special value is available only with listen mode (that is, transports can listen for connections on all network interfaces, but they must connect to a specific interface).
Port | `port` | Required. Specify a port number.
Mode | `mode` | Required. You must select either Connect or Listen from the drop-down menu: connect The transport initiates TCP communication by sending a connection request to <host>:<port>. listen The transport listens for TCP connection requests at <host>:<port>. For more information, see Listen End and Connect End.

See also, Buffer and Performance Settings for Transports.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.