Open topic with navigation

# Configuring Multicast Inbox Communication

Multicast transports can carry one-to-one communication.

Procedure
1. Configure the transport’s multicast groups to support bi-directional communication on the transport bus (see Multicast Transport: Parameters Reference and Multicast Transport: Parameters Reference). The two directions, inbound and outbound, need not use the same multicast group.
2. Select the send inbox and receive inbox abilities for endpoints that use the transport.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.