Open topic with navigation

# Catalog of FTL Server and Service Metrics

This table describes metrics that you can use to assess the operation of the FTL server and services.

## FTL Server Metrics

The sampling interval for FTL server metrics is fixed at 2 seconds. You cannot change this interval.

ID | Metric Type | Description
--- | --- | ---
5009 | Client Connect Count | Cumulative number of client connections since the FTL server process started.
5010 | Client Reconnect Count | Number of clients that reconnected to the FTL server during the sample interval. A spike in this metric could indicate a network connectivity issue between the FTL server and its clients.
5011 | Send to Inbox Failures | Number of undelivered protocol messages that the FTL server sent to a client. A spike in this metric usually indicates that several clients abruptly exited.

## Transport Bridge Metrics

Each bridge is itself an application client, and tracks application metrics; see Catalog of Application Metrics.

The sampling interval for bridge metrics is fixed at 2 seconds. You cannot change this interval.

ID | Metric Type | Description | Tracking
--- | --- | --- | ---
6000 | Bridge Active | 1 indicates that the bridge actively forwards messages. 0 indicates that the bridge is a backup in standby mode. | Per bridge

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO FTL® - Enterprise Edition

Copyright © 2009-2024. Cloud Software Group, Inc. All Rights Reserved.