Open topic with navigation

TIBCO iProcess® Engine 11.9.1

# How BG Processes Send Messages to WIS Processes

The following diagram shows how the `BG` processes send messages to the `WIS` processes using the default configuration.

| 1. | All four `BG` processes are configured to write messages to a single Mbox set, `WMDMBSET`.

| 2. | The `WMDMBSET` Mbox set contains two message queues, `WISMBOX1` and `WISMBOX2`.

| 3. | Both `WISMBD` processes are configured to read messages from the `WMDMBSET` Mbox set. (Each `WISMBD` process then forwards each message to the appropriate `WIS` process via RPC.)

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine

Copyright © 1994-2024. Cloud Software Group, Inc. All Rights Reserved.