Open topic with navigation

TIBCO iProcess® Engine 11.9.1

# WIS_TOUT_GRANULARITY

Draft comments: This parameter is being deleted as a result of the implementation of CR16908

## Section

WQS

## Initial Value

250

## Units

Milliseconds

## Range

>0

## Description

This setting determines the timeout period for the WIS. This effectively sets the granularity of the WIS processes timing. Therefore WIS_RPCSERVICE_PERIOD and WIS_CLIENT_IDLE_PERIOD are only guidelines to the WIS. The WIS will only check the above periods every WIS_TOUT_GRANULARITY milliseconds.For example, if WIS_TOUT_GRANULARITY is set to 2000 and WIS_CLIENT_IDLE_PERIOD set to 500, the effect will be that the WIS_CLIENT_IDLE_PERIOD will be 2 seconds because it will only be checked every 2 seconds.

## Tuning

This should be set in conjunction with the WIS_RPCSERVICE_PERIOD and WIS_CLIENT_IDLE_PERIOD. It should never be greater than WIS_CLIENT_IDLE_PERIOD and for bulk loading it should be the set the same.In general, this should be set to the same value as WIS_CLIENT_IDLE_PERIOD or if less then no less than ¼ of the WIS_CLIENT_IDLE_PERIOD as it causes additional overhead with no benefit.

## Related Parameters

WIS_MAXFILEDESC, WIS_CLIENT_IDLE_PERIOD, WIS_MBOX_WORK_LIMIT.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine

Copyright © 1994-2024. Cloud Software Group, Inc. All Rights Reserved.