Open topic with navigation

TIBCO iProcess® Engine 11.10.0

# MBSET_DEQUEUE_TIMEOUT

Message and Mbox Processing Configuration

## Summary

This attribute defines a time threshold (in milliseconds) for the duration of dequeuing a message from an Mbox set.

If the time for dequeuing the message is equal to or over the defined threshold, the dequeue operation keeps processing, and the time period of dequeuing the message will be logged in the `sw_warn` file. If the time for dequeuing the message is less than the threshold, the dequeue operation will be processed and no log is written in the `sw_warn` file.

## Applies To

This attribute can be set for the `BG` process.

## Permissible Values

The attribute value must be one of the following:

Value | Meaning
n | The timeout threshold, where `n` is any integer value that is 0 - 60000.

## Default Value

The attribute is assigned the following default value when iProcess Engine is installed.

Machine ID | Process | Instance | Value
0 | BG | 0 | 200

## Notes

If you set the value of the attribute to `0`, the time period of dequeuing a message will be logged in the `sw_warn` file each time after dequeuing the message from an Mbox set. This may lead to an extremely large log file, since the log file records each time period of dequeuing messages, which may be problematic.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine

Copyright © 1994-2025. Cloud Software Group, Inc. All Rights Reserved.