Open topic with navigation

TIBCO iProcess® Engine 11.10.0

# WQS_PERSIST_SHMEM

WIS and WQS Process Configuration

## Summary

This attribute defines how often (in seconds) the contents of the `WQS`/`WIS` shared memory are written to the `wqs_index` table in the database.

## Applies To

This attribute can be set for the `WQS` process (only).

## Permissible Values

The attribute value must be an integer in the range 1 to 3600.

## Default Value

The attribute is assigned the following default value when iProcess Engine is installed.

Machine ID | Process | Instance | Value
0 | WQS | 0 | 300

## Notes

When the `WIS` process starts up, it uses the `total_items` column in the `wqs_index` table to determine the number of work items in each work queue. It compares this value to the WIS_CACHE_THRESHOLD value to determine whether to cache the work queue.

If TIBCO iProcess Engine is started, cases are loaded into a work queue, then the system is shut down again within the `WQS_PERSIST_SHMEM` value, the item counts in the `wqs_index` table will not match the actual item counts.

See Configuring When WIS Processes Cache Their Queues for more information.

## See Also

WIS_CACHE_THRESHOLD

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine

Copyright © 1994-2025. Cloud Software Group, Inc. All Rights Reserved.