Open topic with navigation

TIBCO iProcess® Engine 11.10.0

# EMPTYMBOXSLEEP_INC

Message and Mbox Processing Configuration

## Summary

This attribute defines the number of milliseconds or seconds to increment the EMPTYMBOXSLEEP value by when a `BG` or `WISMBD` process requests a message from an empty Mbox.

## Applies To

This attribute can be set for the `BG`, `WISMBD` or ALL processes.

## Permissible Values

The attribute value must be a numeric value in the range 0 to EMPTYMBOXSLEEP_MAX.

## Default Value

The attribute is assigned the following default value when iProcess Engine is installed.

Machine ID | Process | Instance | Value
0 | ALL | 0 | 2

## See Also

EMPTYMBOXSLEEP, EMPTYMBOXSLEEP_MAX

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine

Copyright © 1994-2025. Cloud Software Group, Inc. All Rights Reserved.