# Client Configuration

You can configure TIBCO MFT Platform Server to act as an initiator.

See the following default client (initiator) configuration for TIBCO MFT Platform Server.

    # [ CLIENT ]
    RequiredNodeDefinition: N                                          { N, Y }
    ConnectAdapterIP:       All                         { All, IpName/Address }
    ConnectAdapterIPv6:     All                     { All, IpName/AddressIPv6 }
    TraceLevelClient:       N                    { N, Low|L, Medium|M, High|H }
    TracePathClient:        /mftps/trace/Initiator                  { N, Path }
    TraceSizeClient:        N                                    { N, # of Kb }
    Umask_User:             N                                          { N, Y }
    Timeout:                120                     { Transfer timeout in min }
    DirTransfer0Files:      Failure                    { Failure|F, Success|S }
    RunPPAEndDirTx:         N                                          { N, Y }
    ACCHost:                N                                       { N, Host }
    ACCPort:                9099                                { Port Number }
    ClassOfService:         Default                          { from cfcos.cfg }
    StopOnFailure:          Y                                          { Y, N }

    # SSL Communication. Additional Parameters.
    CertificateFileName:
    PrivateKeyFileName:
    PrivateKeyPwdFileName:
    TrustedAuthorityFileName:
    SSLTraceLevel:          N                                          { N, Y }
    SSLTracePath:           /mftps/trace/SSLInitiator               { N, Path }
    CheckCRL:               N                                          { N, Y }
    CAPath:
    SSLEnabledProtocols:    TLSV1,TLSV1.1,TLSV1.2       {TLSV1,TLSV1.1,TLSV1.2}
    Ciphers:                HIGH                        { openssl_cipher_list }

Copyright © 2022. TIBCO Software Inc. All Rights Reserved.