Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# Defining TIBCO MFT Platform Server for z/OS as a Multi-User Facility

The Platform Server can handle multiple transfers for multiple users simultaneously; therefore, the Platform Server must be defined to CA-Top Secret as a multi-user facility.

You can add the Platform Server as a CA-Top Secret facility by modifying the CA-Top Secret facilities matrix table. This table is contained in the CA-Top Secret `PARMFILE`.

Procedure
1. Add the following entries to your `PARMFILE` to define the Platform Server as a CA-Top Secret facility.

       FAC(USER1=NAME=FUSION)	* Use the USER1 slot
       FAC(FUSION=MULTIUSER) 	* Facility can have multiple users
       FAC(FUSION=AUTHINIT)  	* Facility can issue RACINIT
       FAC(FUSION=PGM=FUS)   	* RACINIT program name starts with FUS
       FAC(FUSION=SIGN(M))   	* Allow multiple signons for the same ACID
       FAC(FUSION=NOLUMSG)	* Do not issue the Last Used message

2. Restart CA-Top Secret to activate previous entries.
   The CA-Top Secret is restarted typically after an IPL. To make these changes dynamically without an IPL, you can enter the following `TSS MODIFY` commands:

       TSS MODIFY(FAC(USER1=NAME=FUSION))
       TSS MODIFY(FAC(FUSION=MULTIUSER))
       TSS MODIFY(FAC(FUSION=AUTHINIT))
       TSS MODIFY(FAC(FUSION=PGM=FUS))
       TSS MODIFY(FAC(FUSION=SIGN(M))
       TSS MODIFY(FAC(FUSION=NOLUMSG))

   In the previous example, `USER1` slot is used in the facilities matrix table and renamed to `FUSION`. You can issue `TSS MODIFY(FAC(FUSION))` to view the facilities matrix table entry to ensure that the entries are installed correctly:

       TSS9550I FACILITY DISPLAY FOR FUSION
       TSS9551I INITPGM=FUS      ID=2  TYPE=099
       TSS9552I ATTRIBUTES=IN-USE,ACTIVE,SHRPRF,ASUBM,NOABEND,MULTIUSER,NOXDEF
       TSS9552I ATTRIBUTES=NOLUMSG,STMSG,SIGN(M),INSTDATA,RNDPW,AUTHINIT
       TSS9552I ATTRIBUTES=NOPROMPT,NOAUDIT,RES,WARNPW,NOTSOC,LCFTRANS
       TSS9552I ATTRIBUTES=MSGLC,NOTRACE,NOEODINIT,IJU,NODORMPW,NONPWR,NOIMSXTND
       TSS9553I MODE=WARN  DOWN=GLOBAL  LOGGING=MSG,SEC9
       TSS9554I UIDACID=8 LOCKTIME=000 DEFACID=*NONE*   KEY=8
       TSS9566I MAXUSER=03000  PRFT=003
       TSS0300I  MODIFY   FUNCTION SUCCESSFUL

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.