Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# SUBDIR={YES | NO | ALL | SEQAVSAM}

Default | `NO`
Allowable Values | `YES` , `NO`, `ALL`, `SEQAVSAM`
Minimum | Not Applicable
Maximum | Not Applicable

This parameter defines whether files within subdirectories are processed. This parameter is used only when directory transfers are performed, and is ignored for non-directory transfer requests.

When a directory structure is defined, this parameter refers to the subdirectories within the directory structure. When z/OS datasets are defined, this parameter defines whether VSAM files or members of a PDS are transferred. For more information of this parameter, see Appendix M. Directory Transfers.

The valid values are as follows:

- `YES`: Sequential and PDS files are selected to be transferred.
- `NO`: Subdirectories are not selected to be transferred.
- `ALL`: Sequential files, PDS files, and VSAM files are selected to be transferred.
- `SEQAVSAM`: Sequential files and VSAM files are selected to be transferred.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.