Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# MQ_WAIT_MSEC

This parameter defines the interval in milliseconds that MQ waits for additional data before returning EOF. If this parameter is not defined, the default value of `5000` is used, which causes MQ to wait for additional data for 5 seconds before returning EOF.

The maximum value allowed is `99999999`. When `0` is specified, MQ does not wait for additional data and returns EOF after reading the last record.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.