Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# Completion of Transfer

The message PGTF3108I is issued at the completion of all file transfer activity. This message can be used for automated processing or scheduling.

Note: The information denoted by the brackets ({ }) are replaceable parameters.

## Successful Completion

`PGTF3108I Transfer {Activity_Number} successfully transferred {Record_Count} records with node:`

`{Remote_Node}{Byte_Count}(Bytes}` or `{Remote_Node}{Member_Count} {Members}`

Where:

- Activity_Number: Indicates the number that is assigned to the transfer.
- Record_Count: Indicates the number of records sent or received by the transaction.
- Remote_Node: Indicates the destination to which you are sending or from which you are receiving a transfer request. This can be displayed as an LU name, IP name, or IP address.
- Byte_Count: Indicates the number of bytes transferred (uncompressed) for a sequential file.
- Member_Count: Indicates the number of members processed for PDS/Library transfers.

`PGTF3108I {Activity_Number} RC={Return_Code} {Remote_Node} {Local_DSN} {Process} Record Count={Record_Count} {S/R} {User_Data}`

Where:

- Activity_Number: Indicates the number that is assigned to the transfer.
- Return_Code: Indicates the number that is returned at the completion of a file transfer. A successful transfer has a return code of all zeroes. An unsuccessful file transfer issues a return code that helps you determine the specific nature of the problem.
- Remote_Node: Indicates the destination to which you are sending or from which you are receiving a transfer request. This can be displayed as an LU name, IP name, or IP address.
- Local_DSN: Indicates the name of the local dataset for the transaction. The dataset name must be a valid z/OS dataset and cannot exceed 54 characters in length. If the dataset provided is invalid, the interface prompts you for a valid name.
- `Process`: Indicates an eight-character description of the transaction being processed.
- Record_Count: indicates the number of records sent or received by the transaction.
- `S/R`: Indicates the direction of the dataset on the host system. For example, if you are sending a file from the Windows system to the host, the direction is `R`.
- User_Data: Indicates the data entered by the user on the PROCESS DESCRIPTION parameter.

## Unsuccessful Completion

`PGTF3109I Activity {Activity_Number} unsuccessful with Node {Remote_Node} Return Code={Return_Code} error type ERROR`

Where:

- Activity_Number: Indicates the number that is assigned to the transfer.
- Remote_Node: Indicates the destination to which you are sending or from which you are receiving a file transfer.
- Return_Code: Indicates the number that is returned at the completion of a file transfer. A successful transfer has a return code of all zeroes. An unsuccessful file transfer issues a return code that helps the user determine the specific nature of the problem.
- Error_Type: Indicates the type of error that caused the transfer to fail.

`PGTF3108I {Activity_Number} RC={Return_Code} {Remote_Node} {Local_DSN} {Process} Record Count={Record_Count} {S/R} {User_Data}`

Where:

- Activity_Number: Indicates the number that is assigned to the transfer.
- Return_Code: Indicates the number that is returned at the completion of a file transfer. A successful transfer has a return code of all zeroes. An unsuccessful file transfer issues a return code that helps you determine the specific nature of the problem.
- Remote_Node: Indicates the destination to which you are sending or from which you are receiving a file transfer.
- Local_DSN: Indicates the name of the local dataset for the transaction. The dataset name must be a valid z/OS dataset and cannot exceed 54 characters in length. If the dataset provided is invalid, the interface prompts you for a valid name.
- `Process`: Indicates an eight-character description of the transaction being processed.
- Record_Count: Indicates the number of records sent or received by the transaction.
- `S/R`: Indicates the direction of the dataset on the host system. For example, if you are sending a file from the Windows system to the host, the direction is `R`.
- User_Data: Indicates the data entered by the user on the PROCESS DESCRIPTION parameter.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.