Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# FUSSUSP

You can use the FUSSUSP exec to suspend an active Platform Server request, and put it in the held status.

## Required Parameter

The following table lists the required parameter of the FUSDEL exec:

Parameter | Description
--- | ---
TRANSN | TRN | Defines the fully qualified transaction number (10 bytes) associated with the request.

## Optional Parameter

The following table lists the optional parameter of the FUSDEL exec:

Parameter | Description
--- | ---
CONFIG | CFG | Defines the configuration file used by the Platform Server exec. If this parameter is not defined, the Platform Server REXX uses the default configuration.

## Return Codes

The return codes of the FUSDEL exec are as follows:

- A zero return code indicates that the Platform Server has suspended the request.

- Non-zero return codes indicate one of the following situations:

  - The Platform Server cannot find the request to be suspended on the active queue.
  - The user is not authorized to suspend the Platform Server request identified by TRANSNUM parameter.
  - The request was in a state that cannot be suspended, such as INACTIVE, HOLD, or DELETE PENDING.
  - A communication error occurred when performing the task.

## Example

The following example shows how to use the FUSSUSP exec to suspend an active Platform Server request:

    FUSSUSP TRANSNUM=IA01500042

The output of the example is as follows:

    retncode===> 0 SUSPEND completed successfully

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.