Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# Enabling Members When GLOBAL AUTOENABLE=NO

When the GLOBAL `AUTOENABLE` parameter is set to `NO`, the members to be enabled are defined by the CONFIG member within the CONFIG DD statement.

The syntax for the CONFIG member is as follows:

    member1,member2
    member3,
     |
     |
    member n

The first member name must start in column 1. Use a comma between member names. If you want to continue to more than one line, you can use more lines. Columns 73 to 80 are ignored. An asterisk (*) in column 1 denotes a comment.

In the following example, three members are enabled at Platform Server initialization:

    *******************************************************************
    * THIS IS WHERE YOU WILL SPECIFY THE OTHER MEMBERS THAT CONTAIN   *
    * CONFIGURATION INFORMATION THAT WILL BE NEEDED TO COMMUNICATE TO *
    * THEM.  THE SAMPLES BELOW SHOULD BE REMOVED AND YOU SHOULD       *
    * SPECIFY THE NAMES THAT YOU HAVE CONFIGURED FOR THE REMOTE       *
    * SYSTEMS IN YOUR NETWORK.                                        *
    *******************************************************************
    SNANODE,                  CONTAINS A SAMPLE OF A REMOTE SNA NODE
    TCPNODE,                  CONTAINS A SAMPLE OF A REMOTE TCP/IP NODE
    DISTRIB                   CONTAINS A SAMPLE OF A LIST OF NODES

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.