Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# Sample FUSCFG Configuration

Member `FUSCFG`, which is a sample shipped with this product, exists in the Platform Server `EXECS` library.

See the following sample `FUSCFG` configuration for your reference.

    *   DEFAULT CONFIGURATION USED IF CONFIG=(OR CFG=) IS NOT ENTERED
    CONFIG=DEFAULT
    STCNAME=FUSION
    AUDPATH1=FUSION.AUDIT.PATH1
    AUDPATH2=FUSION.AUDIT.PATH2

    *   SAMPLE CONFIG FOR STARTED TASK COMMUNICATION WITH FUSION SERVER
    CONFIG=FUSION_STC
    STCNAME=FUSION
    AUDPATH1=FUSION.AUDIT.PATH1
    AUDPATH2=FUSION.AUDIT.PATH2

    *   SAMPLE CONFIG FOR SNA COMMUNICATION WITH FUSION SERVER USING SNA
    CONFIG=FUSION_SNA
    LUNAME=FUSNAPPL
    ACB=FUSN
    *MODENAME=#BATCH

    *   SAMPLE CONFIG FOR TCP COMMUNICATION WITH FUSION SERVER USING IPADDR
    CONFIG=FUSION_IPADDR
    IPADDR=14.0.0.0
    TCPIPJOBNAME=TCPIP
    *IPPORT=46464

    *   SAMPLE CONFIG FOR TCP COMMUNICATION WITH FUSION SERVER USING IPNAME
    CONFIG=FUSION_IPNAME
    IPNAME=NYES9000
    TCPIPJOBNAME=TCPIP
    *IPPORT=46464

The `FUSCFG` configuration member contains the following 5 configurations:

- Default configuration: Defines the default configuration that is set by specifying `CONFIG=DEFAULT`. This configuration is used if the user does not enter the `CONFIG` (`CFG`) parameter on the Platform Server REXX or ISPF Interface. In this case, the default configuration is to use cross memory calls to the Platform Server started task because the `STCNAME` parameter is defined.
- Sample started task configuration: Defines the configuration parameters for communicating with the Platform Server started task through cross memory calls. To use this configuration, you must specify `CONFIG=FUSION_STC` on the command line when you execute a Platform Server client request.
- Sample SNA configuration: Defines the configuration parameters required to communicate with the Platform Server started task through VTAM/SNA services. To use this configuration, you must specify `CONFIG=FUSION_SNA` on the command line when you execute a Platform Server client request.
- Sample TCP IPADDR configuration: Defines the configuration parameters required to communicate with the Platform Server started task through TCP/IP. Using this configuration, the Platform Server REXX attempts to make a connection to the Platform Server at IP address 14.0.0.0 (loopback address). To use this configuration, you must specify `CONFIG=FUSION_IPADDR` on the command line when you execute a Platform Server REXX exec.
- Sample TCP IPNAME configuration: Defines the configuration parameters required to communicate with the Platform Server started task through TCP/IP. Using this configuration, the Platform Server REXX attempts to make a connection to the Platform Server defined to the DNS as NYES9000. To use this configuration, you must specify `CONFIG=FUSION_IPNAME` on the command line when you execute a Platform Server REXX exec.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.