Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# VSAM_RRSLOT={YES | NO}

Default | `NO`
Allowable Values | `YES`, `NO`
Minimum | Not Applicable
Maximum | Not Applicable

This parameter defines whether a RRDS to RRDS file transfer maintains the RRDS slot numbers. This parameter is used only when sending or receiving a RRDS file. When this parameter is defined as `YES`, the Platform Server inserts the RRDS slot number in the first 4 bytes of the record read when sending a RRDS file; the Platform Server is informed that the RRDS slot number is in the first 4 bytes of the record to be written when receiving a record.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.