Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# CHKPT={Y | N | nnn}

Default | `N`
Allowable Values | `Y`, `N`, `nnn`
Minimum | `1`
Maximum | `360`
Alternate Specification | CKPT

You can use this parameter to specify whether to take checkpoints during this transfer. Where, `nnn` specifies the time in minutes that each checkpoint takes. If `Y` is specified, the interval defaults to five minutes.

Note: Checkpoints are taken at time intervals; therefore, you can start a transfer backup at the point of failure if the transfer is interrupted.
Note: Checkpoint restart processing is not supported when spanned files are used (`RECFM=VS` or `RECFM=VBS`).

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.