Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# z/OS Console Display Commands

The z/OS console display command is used to get the information about an executing address space.

Using the console display commands, you can get the following information:

- The started task or job name and the step name
- Whether the job is swapped in, swapped out, or non-swappable
- The user ID assigned to the job
- The started task or job number
- Numbers of the performance group, address space, and domain

To check if the Platform Server is up and running, the console operator must type `D A,jobname`.

See the following sample for the console display:

    JOBS     M/S    TS USERS    SYSAS    INITS   ACTIVE/MAX VTAM     OAS
    00002    00015    00005      00022    00022    00005/00010       00000
     MFTSTC   MFTSTC   STEP1    NSW  S   A=005A   PER=NO   SMC=000
                                         PGN=005  DMN=006  AFF=NONE
                                         CT=011.304S  ET=02.34.54
                                         WUID=STC08893 USERID=MFTSTC
                                         ADDR SPACE ASTE=07763680
                                         DSPNAME=OSIQUEUE ASTE=07791100
                                         DSPNAME=OSIQLOOK ASTE=01C0A900
                                         DSPNAME=OSINODES ASTE=01C0A980
                                         DSPNAME=OSILOGDS ASTE=01C0A800
                                         DSPNAME=OSIWMSGS ASTE=01C0A780

## Platform Server VTAM Tracing

z/OS console operators can turn the VTAM tracing facility on and off by using modify commands. For more information, see Appendix B. Running Traces.

The following DD statement must be included in the startup JCL to enable the tracing facility:

    //VTAMTRAC DD SYSOUT=X

z/OS console operators can turn the SNA packet tracing facility on and off by using the following modify commands:

- `TRON`: To start the SNA packet tracing facility

      F MFTSTC,TRON

- `TROF`: To stop the SNA packet tracing facility

      F MFTSTC,TROF

## Platform Server TCP/IP Tracing

z/OS console operators can turn the TCP/IP tracing facility on and off by using modify commands. The following DD statement must be included in the startup JCL to enable the tracing facility:

    //TCPTRAC DD SYSOUT=X

z/OS console operators can turn the TCP/IP tracing facility on and off by using the following modify commands:

- `TCPTRON`: To start the TCP/IP packet tracing facility

      F MFTSTC,TCPTRON

- `TCPTROF`: to stop the TCP/IP packet tracing facility

      F MFTSTC,TCPTROF

## Platform Server Node Tracing

z/OS console operators can turn the TCP/IP tracing facility on and off by using modify commands. The following DD statement must be included in the startup JCL to enable the tracing facility:

    //TCPTRAC DD SYSOUT=X

z/OS console operators can turn the node tracing on for a particular node defined in the CONFIG by using the following modify commands:

- `TCPTRON`: To start the node tracing facility

      F MFTSTC,TCPTRON,NODENAME

- `TCPTROF`: To stop the node tracing facility

      F MFTSTC,TCPTROF,NODENAME

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.