Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# Appendix A. Sample SNA Mode Definition

The following example is a sample SNA mode definition that is used when working with the Platform Server.

Note: These definitions are not required if you are using the platform server TCP interface.

    USERMODE MODETAB
    *********************************************************************
    *  MODE ENTRIES FOR CYBERFUSION PERFORMANCE BENCHMARKS
    *********************************************************************
    FUSN256 MODEENT LOGMODE=FUSN256, LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                        -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8585',         RUSIZE SEC/PRI  256/256           -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *********************************************************************
    FUSN512 MODEENT LOGMODE=FUSN512, LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                        -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8686',         RUSIZE SEC/PRI  512/512           -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *********************************************************************
    FUSN1K  MODEENT LOGMODE=FUSN1K,  LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                        -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8787',         RUSIZE SEC/PRI 1024/1024          -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *********************************************************************
    FUSN2K  MODEENT LOGMODE=FUSN2K,  LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                                                  -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8888',         RUSIZE SEC/PRI 2048/2048          -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *********************************************************************
    FUSN4K  MODEENT LOGMODE=FUSN4K,  LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                                                  -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8989',         RUSIZE SEC/PRI 4096/4096          -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *********************************************************************
    FUSN8K  MODEENT LOGMODE=FUSN8K,  LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                                                  -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8A8A',         RUSIZE SEC/PRI 8192/8192          -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *
    FUSN16K MODEENT LOGMODE=FUSN16K, LOGON MODE TABLE ENTRY NAME       -
            COS=FAST,                        -
            FMPROF=X'13',            FUNCTION MANAGER PROFILE          -
            TSPROF=X'07',            TRANSMISSION SERVICES PROFILE     -
            PRIPROT=X'B0',           PRIMARY  LOGICAL UNIT PROTOCOL    -
            SECPROT=X'B0',           SECONDARY LOGICAL UNIT PROTOCOL   -
            COMPROT=X'50B1',         COMMON  LOGICAL UNIT PROTOCOL     -
            RUSIZES=X'8B8B',         RUSIZE SEC/PRI 16K (8 X 2**11)    -
            PSNDPAC=5,               PRIMARY  SEND  PACING COUNT       -
            SRCVPAC=5,               SECONDARY RECEIVE PACING COUNT    -
            SSNDPAC=5,               SECONDARY SEND  PACING COUNT      -
            PSERVIC=X'060200000000000000002C00' PRESENTATION SRVCS
    *
    *
            MODEEND
            END

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.