Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# SYSIN Coding Parameters

You can define file transfers by specifying parameters in the SYSIN DD statement.

Note: You can also specify the parameters in the `PARM` field on the JCL EXEC statement. Parameters specified in the `PARM` field override those specified by using the SYSIN DD statement.

The following table lists the parameters that you can specify in a SYSIN DD statement.

Parameter | Alternate Specification | Description
--- | --- | ---
ALLOC_DIR |  | Defines the number of directory blocks for a new file.
ALLOC_PRI |  | Defines the primary allocation quantity for a new file.
ALLOC_SEC |  | Defines the secondary allocation quantity for a new file.
ALLOC_TYPE |  | Defines the type of allocation for a new file.
AVAIL |  | Defines whether TAPE is supported.
BLOCKSIZE | BLKSIZE | Defines the DCB block size for a new file.
CALLJCL |  | Requests the Platform Server to call a user program defined on the remote system with JCL linkage. This parameter should only be used when the remote system is z/OS.
CALLPROG |  | Requests the Platform Server to call a user program defined on the remote system using standard linkage conventions. This parameter should only be used when the remote system is z/OS.
CHKPT | CKPT / CHECKPOINT | Defines the checkpoint interval.
COMPRESS |  | Defines the compression options.
CONTINUE |  | Defines whether transfers continue when a transfer fails.
COSNAME |  | Defines the Class of Service (COS) entry name.
CRCCHECK | CRC | Defines whether CRC checking will be turned on for this transfer.
CRLF |  | Defines the CRLF/LF options.
DATACLASS | DC / DCLASS | Defines the SMS data class.
DATASET_TYPE |  | Defines the type of the new dataset to create.
DATE |  | Defines the date to start the transfer.
DCB |  | Defines RECFM, LRECL, and BLKSIZE.
DCB_LIKE |  | Defines the DCB model DSN.
DESCRIPTION | DESC | Defines the transfer description.
DIRTEST |  | Shows files for a directory transfer.
DSN | LF / LFILE / LDS LOCAL_FILE | Defines the name of the local dataset.
DSORG |  | Defines the dataset organization.
EFFECT |  | Defines the file creation options.
EMAIL_FAIL |  | Defines the email address to which to send an email notification for unsuccessful requests.
EMAIL_GOOD |  | Defines the email address to which to send an email notification for successful requests.
ENCRYPT |  | Defines the data encryption options.
EVERY |  | Defines the repeat cycle of a request.
EVERY_COUNT |  | Defines the number of times that an EVERY request can be scheduled to execute.
EVERY_EXDAYS |  | Defines the EVERY expiration date.
EVERY_EXTIME |  | Defines the EVERY expiration time.
EVERY_MISSED |  | Defines the EVERY control.
EXEC | REXXEXEC / COMMAND | Defines a command or exec for execution on the remote system.
EXECPREPROC |  | Defines whether directory transfer preprocessing actions are executed on the parent transfer or the child transfers. Note: This parameter overrides the value defined in the GLOBAL `EXECPREPROC` parameter.
EXECPOSTPROC |  | Defines whether directory transfer postprocessing actions are executed on the parent transfer or the child transfers. Note: This parameter overrides the value defined in the GLOBAL `EXECPOSTPROC` parameter.
EXPDT |  | Defines the transfer expiration date.
EXPTM |  | Defines the transfer expiration time.
FILEERRORINT |  | Defines the wait interval when a retryable file error occurs. This parameter defines how long a transfer waits before being retried. Note: When defined, this parameter overrides the Node and GLOBAL `FILE_ERROR_TRY_INTERVAL` parameters. When not defined, the GLOBAL FILE_ERROR_TRY_INTERVAL parameters will be used. Note: The actual interval can be up to 60 seconds or more than the value specified, depending on when the error occurs and when the dispatcher runs.
FILEERRORMAX |  | Defines the maximum number of retryable file errors. Note: When defined, this parameter overrides the Node and GLOBAL `FILE_ERROR_TRY_COUNT` parameters. When not defined, the GLOBAL `FILE_ERROR_TRY_COUNT` parameters will be used.
FILE_EXPDT |  | Defines the file expiration date.
FILE_RETPD |  | Defines the file retention period.
HOLD |  | Defines the Hold option.
IPADDR |  | Defines the IP address of the remote system.
IPNAME |  | Defines the IP name of the remote system.
IPPORT |  | Defines the IP port of the remote system.
IUNIT |  | Defines the input tape unit.
IVOLUME |  | Defines the input dataset volume.
LENGTH | LRECL | Defines the DCB logical record length for the new file.
LIST |  | Defines the name of the distribution list.
LOCALLABEL | LLABEL | Defines the label used on the initiating Platform Server when sending or receiving a tape file.
LOCALCTFILE | LCT | Defines the name of the local Translation table.
LOGON_DOMAIN | DOMAIN | Defines the Windows domain where the remote user resides.
LPASS | LOCAL_PASS | Defines the local password.
LUSER | LOCAL_USER | Defines the local user ID.
MAINTAINBDW | MBDW | Defines whether to maintain RECFM=VB BDW when sending or receiving files.
MAINTAINRDW | MRDW | Defines whether to maintain RECFM=VB RDW when sending or receiving files.
MEMBER |  | Defines the member names.
MGTCLASS | MC / MCLASS | Defines the SMS management class
MQ_FAIL |  | Defines the Platform Server to notify MQ on failure.
MQ_GOOD |  | Defines the Platform Server to notify MQ on success.
MQ_NOTIFY |  | Defines when the Platform Server sends MQ notifications.
MQ_WAIT_MESC |  | Defines the number of minutes that MQ waits for data.
NODE |  | Defines the node name of the remote system.
NODECLASS |  | Defines the node class.
NOTIFY |  | Defines the name of the user to notify when the file transfer is completed.
NOTIFY_TYPE |  | Defines the type of user ID to notify.
OVOLUME |  | Defines the output dataset volume.
PASSONLY |  | Defines the Platform Server to encrypt only the password.
PERMIT_ACTNS |  | Defines the Windows-permitted actions.
POST_ACTION | PPA | Defines the postprocessing action.
PRIORITY |  | Defines the transfer schedule priority.
PROCNAME |  | Defines the process name.
PURGE |  | Defines the timeout request option.
RDSIP |  | Defines the remote file disposition.
RECFM |  | Defines the DCB record format for the new file.
REMOTECTFILE | RCT | Defines the name of the remote Translation table.
REMOTELABEL | RLABEL | Defines the label used on the responder Platform Server when sending or receiving a tape file.
REMOTE_FILE | RF / RFILE / RDSN | Defines the name of the file on the remote system.
REMOTE_PASS | RPASS | Defines the password for the remote user on the remote system.
REMOTE_UNIT | UNIT | Defines the unit for file creation.
REMOTE_USER | RUSER | Defines the name of the user on the remote system.
REMOVETRAIL | RMTRAIL | Defines whether to remove trailing blanks and nulls.
RESOLVE_GDG |  | Defines the GDG resolution indicator.
RETENTIONPRD |  | Defines the retention period for the transfer request.
RETRY | TRY | Defines the number of times that a request will be tried.
RETRYINT |  | Defines the retry interval.
RMTRAIL |  | Defines whether to remove the trailing spaces.
RSACCELERATOR | RSA | Defines whether transfers go to an RSA host.
RSCOMPRESS | RSC | Defines whether RSA uses compression.
RSENCRYPT | RSE | Defines whether RSA uses encryption.
RSHOST | RSH | Defines the RSAccelerator host name or IP address.
RSMAXSPEED | RSMAX | Defines the maximum speed that RSA uses.
RSPORT |  | Defines the RSAccelerator port number.
RSPROTOCOL | RSP | Defines the protocol that RSA uses.
SCRIPT |  | Defines the name of the script file in the started task.
SENDRECFMU |  | Defines whether to maintain RECFM=VB BDW when sending or receiving files.
SPACE |  | Defines the space for a new file.
SPACERELEASE |  | Defines the release unused space flag.
SSL |  | Defines the SSL options. SSL is now an alias of the TLS parameter. See the TLS parameter.
SPACE |  | Defines the space for a new file.
SPACERELEASE |  | Defines the release unused space flag.
STORCLASS | SC / SCLASS | Defines the SMS storage class.
SUBDIR |  | Defines whether to use subdirectories.
SUBMIT |  | Defines the Platform Server to submit JCL to the remote system.
TAPE |  | Notifies the Platform Server that this is an uncatalogued tape transfer.
TCP_TIMEOUT | TCPTIMEOUT | Defines the TCP timeout, in minutes, for this transfer. Note: This parameter overrides the TCP_TIMEOUT defined in the GLOBAL configuration.
TEMPLATE |  | Defines the Windows template.
TEXTEOFTERM |  | Defines the CRLF/LF end of file options.
TIME |  | Defines the time at which to start a transfer.
TLS |  | Defines whether TLS is used for the request. (SSL is now an alias of the TLS parameter.)
TRANS_TYPE |  | Defines the transfer type.
TRANSFER |  | Defines the file transfer direction.
TRCLASSNAME | TRCLASS | Defines the transfer class.
TRUNCATE |  | Defines the truncation options when receiving a file from Windows, UNIX, IBM i, or MFT Internet Server when record delimiters are defined.
TYPE |  | Defines the TEXT or BINARY file.
UNIXPERM |  | Defines the permissions that are set when you create a file on a target UNIX system.
UTF8BOM |  | Defines whether the UTF-8 BOM (0xefbbbf) is added at the start of the converted data or is removed from the start of the data before conversion.
VOLUME | VOL / VOLSER | Defines the volume for file creation.
VSAM_KEYLEN |  | Defines the VSAM KSDS key length.
VSAM_KEYPOS |  | Defines the VSAM KSDS relative key position.
VSAM_LIKE |  | Defines the VSAM model DSN.
VSAM_LRECL |  | Defines the VSAM record length.
VSAM_RRSLOT |  | Defines the VSAM RRDS slot number option.
VSAM_REUSE |  | Defines the VSAM REUSE option.
VSAM_TYPE |  | Defines the VSAM file organization.
WAIT |  | Defines the transfer WAIT options.
XMEMBER |  | Defines the excluded member names.

Subtopics

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.