Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# SENDERCFMU={YES | NO | NOBDW}

Default | None
Allowable Values | `YES`, `NO`, `NOBDW`
Minimum | Not Applicable
Maximum | Not Applicable

This parameter defines whether to maintain RECFM=VB BDW when sending or receiving files.

The valid values are as follows:

- `YES`: When `YES` is specified for a send file transfer, the file is opened using `RECFM=U`. Each block is written as an individual record. The main use of this parameter is to retain the `RECFM=VB` block and record structure when sending a file to a UNIX or Windows platform.
- `NO`: When `NO` is specified for a send file transfer, the file is not opened using `RECFM=U`. The default value is `NO`.
- `NOBDW`: When `NOBDW` is specified for a send file transfer, the file is opened using `RECFM=U`. Each block is written as an individual record. This parameter is the same as `YES`, except that the `BDW` is not sent.

Note: This parameter must be used only when `TYPE=BINARY` is specified.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.