Open topic with navigation

TIBCO® Managed File Transfer Platform Server for z/OS 8.1.0

# RSMAXSPEED

When you conduct file transfers through an RSAccelerator (RSA), this parameter defines the maximum speed in Kilobytes per second to be used by the RSA server when you set this parameter in your command line or transfer template. This parameter can be 256 - 100000 kbps.

Copyright © 2003-2021. TIBCO Software Inc. All Rights Reserved.